**OM-RI-09 0151.00-SUP.docx**

**REHABILITATION OF ACOUSTICAL CEILING TILE**

|  |  |  |
| --- | --- | --- |
| **SECTION USAGE MATRIX** | | |
| C | NA | Seminary and Small Institute Standard Plan (CHURCH EDUCATION SYSTEM) - New Project |
| SM | NA | Standard MEETINGHOUSE and PHASED MEETINGHOUSE Standard Plan - New Project |
| R | SUP | OM/RI (REPLACEMENT & IMPROVEMENT) for Existing Meetinghouse / Seminary and Institute Project |
| CM | NA | Meetinghouse and Phased Meetinghouse Standard Plan with S&I MODULE ADDITION - New Project |
| SI | NA | S&I MODULE Addition to Existing Meetinghouse Building |
| MO | NA | MISSION OFFICE MODULE Addition to Existing Meetinghouse Building |
| UM | NA | URBAN MEETINGHOUSE for Custom Meetinghouse - New or Addition Project |
| FM | NA | Small Maintenance Project specification for FACILITY MANAGER |
|  |  |  |

|  |  |  |
| --- | --- | --- |
| **MODIFICATION LOG** | | |
| DATE | SOURCE | DESCRIPTION |
|  |  |  |
|  |  |  |

SECTION 09 0151

REHABILITATION OF ACOUSTICAL CEILING TILE

1. GENERAL
   * + 1. SUMMARY
          1. Includes But Not Limited To:

**EDIT REQUIRED:** List or describe existing interior areas where acoustical tile surfaces are to be finished under this Section, show them graphically on the Drawings, or include them in a schedule on the Drawings. If one of the latter two options is used, delete subparagraph below.

Prepare and paint existing ceiling tile in following areas as described in Contract Documents:

<**Insert Areas where Ceiling Tile is to be Painted**>.

<**Insert Areas where Ceiling Tile is to be Painted**>.

<**Insert Areas where Ceiling Tile is to be Painted**>.

* + - * 1. Related Requirements:

Section 09 9001: Common Painting Requirements.

1. PRODUCTS
   * + 1. SYSTEM
          1. Description:

Use MPI(a) INT 9.3A Latex Finish system.

* + - * 1. Performance:

Gloss / Sheen Level Required: Gloss Level 1.

* + - * 1. Materials:

Type Two Acceptable Stain Blocker (If necessary):

Benjamin Moore: 023 Fresh Start.

ICI Paints:

ICI Dulux: 3210-XXXX Gripper Aquacrylic Primer / Sealer.

ICI Devoe: 51801 Kilstain W / B Primer Sealer.

ICI Fuller O'Brien: PrimZ Interior / Exterior Primer Sealer.

PPG Paints:

PPG Pittsburgh Paints: 17-21 Seal-Grip Stain Blocker Primer.

PPG Porter: 1129 Blankit Interior Acrylic Primer / Sealer.

Pratt & Lambert.

Sherwin-Williams.

Wm. Zinsser.

Equal as approved by Architect before use. See Section 01 6200.

Category Four Approved Products. See Section 01 6200 for definitions of Categories.

Products listed in edition of MPI Approved Product List current at time of bidding and later are approved, providing they meet VOC requirements in force where Project is located.

Finish Coat:

MPI Product 53.

1. EXECUTION
   * + 1. APPLICATION
          1. See appropriate paragraphs of Section 09 9001.
          2. Clean acoustic tile surface and prepare as recommended by Paint Manufacturer. In addition, apply shellac or a stain blocker as recommended by Finish Coat Manufacturer over dirty or stained areas.
          3. Apply finish coat as follows:

Perforated tile: Roll or spray.

Fissured tile: Spray only.

END OF SECTION