**OM-RI-09 0171.00-SUP.docx**

**REHABILITATION OF SISAL WALL COVERING**

|  |  |  |
| --- | --- | --- |
| **SECTION USAGE MATRIX** | | |
| C | NA | Seminary and Small Institute Standard Plan (CHURCH EDUCATION SYSTEM) - New Project |
| SM | NA | Standard MEETINGHOUSE and PHASED MEETINGHOUSE Standard Plan - New Project |
| R | SUP | OM/RI (REPLACEMENT & IMPROVEMENT) for Existing Meetinghouse / Seminary and Institute Project |
| CM | NA | Meetinghouse and Phased Meetinghouse Standard Plan with S&I MODULE ADDITION - New Project |
| SI | NA | S&I MODULE Addition to Existing Meetinghouse Building |
| MO | NA | MISSION OFFICE MODULE Addition to Existing Meetinghouse Building |
| UM | NA | URBAN MEETINGHOUSE for Custom Meetinghouse - New or Addition Project |
| FM | NA | Small Maintenance Project specification for FACILITY MANAGER |
|  |  |  |

|  |  |  |
| --- | --- | --- |
| **MODIFICATION LOG** | | |
| DATE | SOURCE | DESCRIPTION |
|  |  |  |
| 17 Jul 14 | Greg Adams | Approved Manufacture updated. |
| 28 Feb 13 | Gail Olsen | Removed Reference Standard and Regulatory Agency requirements. General Upgrade. |
| 26 Oct 10 | Gail Olsen | Reference Standard and Regulatory Agency updated for Canada. General Upgrade. |
| 29 Apr 09 | Michael Jenson | Major Upgrade. |
| 04 Apr 09 | Gail Olsen | Reference Standard updated. |
| 31 May 05 | Michael Jenson | New Section. |

SECTION 09 0171

REHABILITATION OF SISAL WALL COVERING

1. GENERAL
   * + 1. SUMMARY
          1. Includes But Not Limited To:

EDIT REQUIRED: List or describe existing interior areas where sisal wall covering surfaces are to be finished under this Section, show them graphically on Drawings, or include them in a schedule on Drawings. If one of the latter two options is used, delete subparagraph below.

Prepare and colourize existing sisal wall covering in following areas as described in Contract Documents:

<Insert Areas where Sisal Wall Covering is to be rehabilitated>.

<Insert Areas where Sisal Wall Covering is to be rehabilitated>.

<Insert Areas where Sisal Wall Covering is to be rehabilitated>.

* + - 1. SUBMITTALS
         1. Action Submittals:

Samples: One foot square (0.093 sq m) samples of standard LDS colors from the Church of Jesus Christ of Latter-day Saints.

* + - * 1. Informational Submittals:

Qualification Statements:

Approved Applicator’s written affirmation that those applying system have received training acceptable to Manufacturer / Licensor and that specialized equipment acceptable to Manufacturer / Licensor will be used in application of system.

* + - * 1. Closeout Submittals:

Include following in Operations And Maintenance Manual specified in Section 01 7800:

Warranty Documentation:

Final, executed copy of Warranty.

* + - 1. DELIVERY, STORAGE, AND HANDLING
         1. Delivery And Acceptance Requirements:

Deliver materials in sealed containers with Manufacturer’s labels intact.

* + - * 1. Storage And Handling Requirements:

Store materials in protected area at temperatures below 90 deg F (32 deg C) and above 50 deg F (10 deg C). Keep from freezing.

Keep container tightly closed in a well ventilated area, and store upright when not in use.

Shelf life: One (1) year minimum - Unopened containers.

* + - 1. FIELD CONDITIONS
         1. Ambient Conditions:

Apply when the temperature is between 50 deg F (10 deg C) minimum and 100 deg F (38 deg C) maximum and relative humidity is less than seventy five (75) percent.

Provide good ventilation.

* + - 1. WARRANTY
         1. Manufacturer Warranty:

Provide five (5) year warranties as follows:

From applicator for proper installation.

From Manufacturer for color retention.

1. PRODUCTS
   * + 1. SYSTEM
          1. Manufacturers:

Approved Manufacturers:

Category One VMR Approved Manufacture and product. See Section 01 6200 for definition of Categories:

Newcolour by Wilson & Hampton Inc, Anaheim, CA [www.NewColourSisal.com](http://www.NewColourSisal.com).

Category Four Approved System. See Section 01 6200 for definition of Categories:

Approved process by Sisal Restoration Systems, Riverside, CA [www.SisalRestorationSystems.com](http://www.SisalRestorationSystems.com).

* + - * 1. Materials:

EDIT REQUIRED: Include following paragraph if mildew is present.

Provide Manufacturer’s specified anti-mildew additive.

1. EXECUTION
   * + 1. EXAMINATION
          1. Verification Of Conditions:

Examine wall covering to receive colourant system and report in writing conditions that would adversely affect appearance or performance of system which cannot be put into acceptable condition by specified surface preparation.

* + - 1. PREPARATION
         1. All surfaces must be sound, clean and free from oil, grease, dirt, mildew, loose or flaking paint/sisal, and any other foreign substances.
         2. Mask off, remove, or otherwise protect surfaces and items not to receive colourant system.
         3. Clean wall covering surface and prepare as recommended by System Manufacturer. In addition, spot prime discolored or water-stained areas as recommended by System Manufacturer. Some stains may require a second coat.
      2. APPLICATION
         1. Apply specified system using Manufacturer / Licensor’s recommended equipment and following Manufacturer / Licensor’s application recommendations.

END OF SECTION